Chapter 2: Heating Load Estimates

TRUE/FALSE

	1.	The design heating load of a building is an estimate of the rate at which a building loses heat during the near minimum outdoor temperature.

ANS:	T	PTS:	1	REF:	22

	2.	One can assume that individual room heating loads are proportional to room floor area.

ANS:	F	PTS:	1	REF:	22

	3.	The R-value of a material is not directly proportional to its thickness.

ANS:	F	PTS:	1	REF:	24

	4.	Many residential and commercial buildings have concrete floor slabs rather than crawl spaces or full basements.  Downward heat losses are relatively small from interior areas of the floor slab.

ANS:	T	PTS:	1	REF:	29-30

	5.	The U-value of any material or assembly is simply the reciprocal of the R-value of that material or assembly.

ANS:	T	PTS:	1	REF:	31

	6.	Heat is lost through all building surfaces that separate heated space from unheated space.

ANS:	T	PTS:	1	REF:	31

	7.	It is relatively easy to assess the location and magnitude of all the air leakage paths in a typical building.

ANS:	F	PTS:	1	REF:	32

	8.	The number of heating degree days that accumulate in a 24-hr. period is the difference between 72 F and the average outdoor air temperature during that period.

ANS:	F	PTS:	1	REF:	42-43

	9.	Knowing how many MMBtu a building requires over a typical heating season is not of much use to most owners.

ANS:	T	PTS:	1	REF:	45

	10.	A boiler, furnace, or small space heater operating on the same fuel, at the same assumed conversion efficiency, would produce the same estimated annual heating cost.

ANS:	T	PTS:	1	REF:	47

MULTIPLE CHOICE

	1.	The heating load is ____ of heat flow from the building to the outside air.
a.	a rate	c.	the cost	
b.	the quantity	d.	one unit	

ANS:	A	PTS:	1	REF:	22

	2.	The proper approach is to perform a heat load calculation ____.
a.	factoring seasonal requirements	c.	for the entire building	
b.	for each room	d.	based on the owner’s usage	

ANS:	B	PTS:	1	REF:	22

	3.	An object’s thermal ____ can be defined as its thickness in the direction of heat flow divided by its thermal conductivity.
a.	reactivity	c.	reciprocity	
b.	reproduction	d.	resistance	

ANS:	D	PTS:	1	REF:	23

	4.	Heat flow from a basement or slab-on-grade foundation is determined by complex interactions between the building, the surrounding soil, insulation materials (if present), and the ____.
a.	depth of the foundation	c.	air temperature above grade	
b.	orientation of the structure	d.	planned usage of the room	

ANS:	C	PTS:	1	REF:	26

	5.	All building surfaces that separate heated space from unheated space. (walls, windows, ceilings, doors, foundation, etc.) are called the ____ of the building.
a.	thermal envelope	c.	resistance factors	
b.	heat load variables	d.	thermal qualifiers	

ANS:	A	PTS:	1	REF:	31-32

	6.	The U-value of any material or assembly is simply the reciprocal of the ____ of that material or assembly.
a.	heat load	c.	exposure	
b.	temperature	d.	R-value	

ANS:	D	PTS:	1	REF:	31

	7.	In addition to conduction losses, heat is also carried out of buildings by uncontrolled air leakage. This is called ____ heat loss.
a.	anti-thermal	c.	insulation	
b.	infiltration	d.	environmental	

ANS:	B	PTS:	1	REF:	32

	8.	One common method of factoring local weather conditions into estimates of heating energy use is based on heating ____.
a.	prognostication	c.	historical records	
b.	thermometers	d.	degree days	

ANS:	D	PTS:	1	REF:	42

	9.	Once the____ price of the fuel options has been calculated, a simple multiplication determines the estimated seasonal heating cost in dollars.
a.	effective	c.	advertised	
b.	unit	d.	estimated	

ANS:	B	PTS:	1	REF:	45

	10.	To estimate the annual space heating cost provided by an electrically operated heat pump, its average COP must be factored in.  What does COP stand for?
a.	coefficient of performance	c.	calculation of price	
b.	capacity of production	d.	correlation of parts	

ANS:	A	PTS:	1	REF:	45